csx equipment defect detector milepost 0 39 track 1 first clearance defect from axle 60 to axle 61 second clearance defect near axle 95 third clearance defect from axle 98 to axle 101 fourth clearance defect from axle 110 to axle 113 defects inspect train total axles 136 out
